Marcel Galliker

marcel@radex-net.com

A short introduction to install Windows 7 Embedded.

Ergosoft Rip  
Installation

Documentation

Version 0.0.0.1

Contents

[1 Introduction 2](#_Toc420426571)

[2 Directories on RIP-Server 2](#_Toc420426572)

[3 Directories on Printer 3](#_Toc420426573)

[4 User Directory 4](#_Toc420426574)

[5 Ergosoft Options 4](#_Toc420426575)

[6 Hotfolder 6](#_Toc420426576)

[7 Print Environment 7](#_Toc420426577)

# Introduction

This manual shows how to install and setup the Ergosoft Rip on a Windows Server.

# Directories on RIP-Server

There are two ways of where the Source Data is stored.

1. On the RIP-Server
2. On the Printer

On both PCs there is a shared Folder D:\SourceData. The can be configured to use one of them as tis Source Data directory.

|  |  |
| --- | --- |
|  | |
| Directories:   * D:\Ergosoft * D:\Ergosoft\User * D:\Ergosoft\Hotfolder * D:\SourceData | (local)  (local) User Data  (local) Data for HotFolder  Shared network folder. |
| Sharing the folder D:\SourceData  Click on <Advanced Sharing> | |
| Select <Share this folder> as <SourceData>.  Permissions can stay on the default setting. (Probably ) | |

# Directories on Printer

|  |  |
| --- | --- |
| D:\SourceData | Shared on the network as “SourceData” |
| D:\PrintData\ | Shared on the network as “PrintData”. The RIP-Server has writing permits. |
| D:\PrintData\<printenv..x> | One directory per print environment. |

# User Directory

|  |
| --- |
| Start the Ergosoft Maintenance Tool and click on <Set user data path> |
| Select <Change folder> and set the folder to D:\Ergosoft\User. |

# Ergosoft Options

The following are settings on the Ergosoft “Options” menu that differ from the default settings

|  |
| --- |
| Print Marks: Deselect all! |
| Color Management/Input Profile: Do not ask user! |
| Application / Spectrophotometer: Do not use Print Marks! |

# Hotfolder

|  |
| --- |
| Setup the Ergosoft Hotfolder like this.  Important: it must be **<ONLINE>.** |

# Print Environment

|  |
| --- |
| The names of the print environment are defined as:  <printer> - <environment>  Example: “Printer 1 – 4C Tiff” |
| On Printer: Create Directory D:\PrintData\<PrintEnv> |
| On Texprint: Click <Add new Print Environment>  On Print Environment: Click <Add> |
| Click on <+> |
| Select the driver corresponding your count out of Ergosoft / Test TIFF Rester Mono. |
| Click on <Add Port> |
| Select <File Intterface> and click on <OK>. |
| Type in the path to the PrintData folder on the printer. Using a fixed IP-Address speeds up network connection.  Click on <OK>.  Click on <OK>. |
| Type in your print environment name and click <OK>. |
| Type in your print environment name and click <OK>. |
| Set the Device Options as follows (dpi may vary). |
| Set the “Printing Ink Assignment” according to your printer setup. |